Author: Steve Platt

Nutexa
HM2100
High Performance Premium

Technical
Information

HM2100 is recommended for use on Trailers and semi- trailers.
It has excellent resistance to fading, high performance and an optimal compatibility with the brake drum.

Gliding speed: 18 m/s
Working temperatures:
Operating temperature: 250°C
Short time temperature: 450°C
Friction Coefficent
Classification
Normal : G
Hot: G
Wear rate: Cm³/Kwh: 0.177

Nutexa Frictions Ltd
New Hall Lane, Hoylake, Wirral, CH47 4BP, ENGLAND
Tel 0151 632 5903 Fax 0151 632 5908
E-mail: sales@nutexafrictions.co.uk Web site: www.nutexafrictions.co.uk