Author: Steve Platt

Nutexa
HM2200
High Performance Premium

Technical
Information

HM2200 is recommended for use on Trucks, Buses and Coaches.
It has excellent resistance to fading, high performance and an optimal compatibility with the brake drum. It has high efficiency over a broad temperature range.

Gliding speed: 15m/s
Working temperatures:
Operating temperature: 250°C
Short time temperature: 500°C
Friction Coefficient
Classification
Normal : G
Hot: G
Wear rate: Cm³/Kwh: 0.204

Nutexa Frictions Ltd
New Hall Lane, Hoylake, Wirral, CH47 4BP, ENGLAND
Tel 0151 632 5903 Fax 0151 632 5908
E-mail: sales@nutexafrictions.co.uk Web site: www.nutexafrictions.co.uk