Author: Steve Platt

Nutexa
HM1200
High Performance Premium

Technical
Information

HM1200 is a medium friction asbestos free brake lining incorporating a fibreglass base. This lining is recommended for use on trucks, tractor units, buses, and semi-trailers.
This virtually noise free, top premium mix shows stable braking power, long life and
exceptional drum compatibility, with a swell factor to avoid any possibility of wheel lock-up.
Performance and wear qualities are proven by millions of miles of practical use. High
structural strength avoids cracking or disintegration. HM1200 has been particularly
successful in overcoming squeal and short life on buses and coaches operating in
congested city traffic.
HM1200 is a top quality lining, which is recommended to meet all your requirements.

Nutexa Frictions Ltd
New Hall Lane, Hoylake, Wirral, CH47 4BP, ENGLAND
Tel 0151 632 5903 Fax 0151 632 5908
E-mail: sales@nutexafrictions.co.uk Web site: www.nutexafrictions.co.uk